Summary of Changes

Effective Monday, March 21, 2106, CenturyLink will implement Version 52 of the Access Services Ordering Guidelines within its Pre-Order and Ordering Interface systems.

During the release implementation, EASE VFO (Virtual Front Office) and UOM (Unified Ordering Model) will be unavailable for processing transactions from 5:00 PM ET on Friday, March 18th, 2016 until 7:00 AM ET on Monday, March 21, 2016.

CenturyLink will modify product based edits including, but not limited to, the following:

*Please NOTE: A complete list of EASE custom edits can be viewed by clicking on the web-link for ASR CenturyLink Custom Business Rules available from the EASE Homepage in the Guide (ASR) TAB.*

| **Action** | **ASR Form** | **Field** | **Business Rule / WEBCALL / EDIT** | **Error Code** |
| --- | --- | --- | --- | --- |
| Add | TRANS | GETO | TRANS GETO OF F ONLY ALLOWED WHEN OTC IS NOT CENTURYLINK | EQ882 |
| Add | ASR | SPEC | ASR SPEC MUST EQUAL ETHTSAA WITH NC CODE PROVIDED | EQ886 |
| Add | ASR | SPEC | ASR SPEC MUST EQUAL GEOMAX OWSPL OR ETHTSAA WHEN NC KRRG | EQ887 |
| Add | EVC | AUNT | ONE OCCURRENCE OF THE EVC.EVC\_DETAILS.UNI\_MAPPING.AUNT FIELD MUST BE POPULATED WHEN ASR.ACT IS N OR R AND ASR.EVCI IS B | EQ888 |
| Add | EVC | AUNT | ONE OCCURRENCE OF THE EVC.EVC\_DETAILS.UNI\_MAPPING.AUNT FIELD MUST BE POPULATED WHEN ASR.ACT IS D AND ASR.EVCI IS B | EQ889 |
| Add | EVC | AUNT | ONLY ONE OCCURRENCE OF THE EVC.EVC\_DETAILS.UNI\_MAPPING.AUNT FIELD CAN BE POPULATED WHEN ASR.EVCI IS B | EQ890 |
| Add | TRANS | SECLOC | TRANSPORT SECLOC POSTION 1 OF E IS NOT ALLOWED TO BE CHANGED ON SUP 3 | EQ891 |
| Add | SALI |  | ADDRESS DOES NOT VALIDATE. PLEASE VERIFY ADDRESS DETAILS AND OTC FIELD VALUE. | CTLV0004 |
| Add | EVC | EVCID | EVCID FOUND EXISING IN INVENTORY | CTLV0086 |
| Add | CLLI |  | GIVEN ADDRESS IS NO MATCH | CTLV0155 |
| Add | ASR | ASC-EC | ASC-EC FIELD AND MULTI-EC FORM REQUIRED. BASED ON ASR DATA | CTLV0202 |
| Change | RING | PORTS | THIS FIELD IS REQUIRED. | EQ006 |
| Change | EUSA | PSPEED | PSPEED VALID VALUES = 56K, 64K, 1.544M, 128K, 256K, 384K OR 12M; BASED ON NC | EQ30 |
| Change | ASR | PROJECT | ASR ADMIN PROJECT MUST BEGIN WITH NATE, ENET , or CNDC | EQ517, EQ518, EQ519, EQ520, EQ521, EQ522, EQ523, EQ524 |
| Change | TRANS | SECLOC | TRANSPORT SECLOC POSTION 1 OF E IS NOT ALLOWED TO BE CHANGED ON SUPS | EQ544 |
| Change | TRANS | NCI | IF TRANSPORT / ACI CCEA IS POPULATED THE 3and 4 POSITION OF THE TRANSPORT NCI MUST EQUAL QB | EQ663 |
| Change | ASR | SPEC | ASR SPEC MUST EQUAL OWSP1 OR GEOMAX ON OWS AND GEOMAX PONS | EQ737, EQ739 |
| Change | ASR | SPEC | ASR SPEC MUST EQUAL GEOMAX ON GEOMAX PONS | EQ740, EQ741, EQ742 |
| Change | EVC | LREF | PERFORMANCE MONITORING EVCPM REQUIRED IN LOS OF AT LEAST ONE LREF 2 | EQ793, EQ794 |
| Change | EVC | RPON | THE EVC RPON IS NOT ALLOWED WHEN THE UACT IS C, D, N OR R | EQ876 |
| Change | TRANS | SCFA | ACTL IN SECLOC AND 1st 8 OF MUX IN SMUXLOC RQD WITH SCFA | EQWS293 |
| Change | SALI |  | ADDRESS IS NOT VALID | CTLV0004 |
| Remove | EVC | RUID | THE EVC RPON IS NOT ALLOWED WHEN THE RUID IS POPULATED ALSO | EQ877 |